NPS Network Processor

Required properties:

- compatible :	should be "ezchip,nps400-timer1"

Clocks required for compatible = "ezchip,nps400-timer1":
- clocks : Must contain a single entry describing the clock input

Example:

timer {
	compatible = "ezchip,nps400-timer1";
	clocks = <&sysclk>;
};
