Analog Devices SSM2305 Speaker Amplifier
========================================

Required properties:
  - compatible : "adi,ssm2305"
  - shutdown-gpios : The gpio connected to the shutdown pin.
                     The gpio signal is ACTIVE_LOW.

Example:

ssm2305: analog-amplifier {
	compatible = "adi,ssm2305";
	shutdown-gpios = <&gpio3 20 GPIO_ACTIVE_LOW>;
};
