// SPDX-License-Identifier: GPL-2.0-only
/*
 * Device Tree Source for AM33xx clock data
 *
 * Copyright (C) 2013 Texas Instruments, Inc.
 */
&scm_clocks {
	sys_clkin_ck: clock-sys-clkin-22@40 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "sys_clkin_ck";
		clocks = <&virt_19200000_ck>, <&virt_24000000_ck>, <&virt_25000000_ck>, <&virt_26000000_ck>;
		ti,bit-shift = <22>;
		reg = <0x0040>;
	};

	adc_tsc_fck: clock-adc-tsc-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "adc_tsc_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dcan0_fck: clock-dcan0-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dcan0_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dcan1_fck: clock-dcan1-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dcan1_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	mcasp0_fck: clock-mcasp0-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "mcasp0_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	mcasp1_fck: clock-mcasp1-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "mcasp1_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	smartreflex0_fck: clock-smartreflex0-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "smartreflex0_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	smartreflex1_fck: clock-smartreflex1-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "smartreflex1_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	sha0_fck: clock-sha0-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "sha0_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	aes0_fck: clock-aes0-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "aes0_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	rng_fck: clock-rng-fck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "rng_fck";
		clocks = <&sys_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	clock@664 {
		compatible = "ti,clksel";
		reg = <0x664>;
		#clock-cells = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		ehrpwm0_tbclk: clock-ehrpwm0-tbclk@0 {
			reg = <0>;
			#clock-cells = <0>;
			compatible = "ti,gate-clock";
			clock-output-names = "ehrpwm0_tbclk";
			clocks = <&l4ls_gclk>;
		};

		ehrpwm1_tbclk: clock-ehrpwm1-tbclk@1 {
			reg = <1>;
			#clock-cells = <0>;
			compatible = "ti,gate-clock";
			clock-output-names = "ehrpwm1_tbclk";
			clocks = <&l4ls_gclk>;
		};

		ehrpwm2_tbclk: clock-ehrpwm2-tbclk@2 {
			reg = <2>;
			#clock-cells = <0>;
			compatible = "ti,gate-clock";
			clock-output-names = "ehrpwm2_tbclk";
			clocks = <&l4ls_gclk>;
		};
	};
};
&prcm_clocks {
	clk_32768_ck: clock-clk-32768 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "clk_32768_ck";
		clock-frequency = <32768>;
	};

	clk_rc32k_ck: clock-clk-rc32k {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "clk_rc32k_ck";
		clock-frequency = <32000>;
	};

	virt_19200000_ck: clock-virt-19200000 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "virt_19200000_ck";
		clock-frequency = <19200000>;
	};

	virt_24000000_ck: clock-virt-24000000 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "virt_24000000_ck";
		clock-frequency = <24000000>;
	};

	virt_25000000_ck: clock-virt-25000000 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "virt_25000000_ck";
		clock-frequency = <25000000>;
	};

	virt_26000000_ck: clock-virt-26000000 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "virt_26000000_ck";
		clock-frequency = <26000000>;
	};

	tclkin_ck: clock-tclkin {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-output-names = "tclkin_ck";
		clock-frequency = <12000000>;
	};

	dpll_core_ck: clock@490 {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-core-clock";
		clock-output-names = "dpll_core_ck";
		clocks = <&sys_clkin_ck>, <&sys_clkin_ck>;
		reg = <0x0490>, <0x045c>, <0x0468>, <0x0460>, <0x0464>;
	};

	dpll_core_x2_ck: clock-dpll-core-x2 {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-x2-clock";
		clock-output-names = "dpll_core_x2_ck";
		clocks = <&dpll_core_ck>;
	};

	dpll_core_m4_ck: clock-dpll-core-m4@480 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_core_m4_ck";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <31>;
		reg = <0x0480>;
		ti,index-starts-at-one;
	};

	dpll_core_m5_ck: clock-dpll-core-m5@484 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_core_m5_ck";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <31>;
		reg = <0x0484>;
		ti,index-starts-at-one;
	};

	dpll_core_m6_ck: clock-dpll-core-m6@4d8 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_core_m6_ck";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <31>;
		reg = <0x04d8>;
		ti,index-starts-at-one;
	};

	dpll_mpu_ck: clock@488 {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-clock";
		clock-output-names = "dpll_mpu_ck";
		clocks = <&sys_clkin_ck>, <&sys_clkin_ck>;
		reg = <0x0488>, <0x0420>, <0x042c>, <0x0424>, <0x0428>;
	};

	dpll_mpu_m2_ck: clock-dpll-mpu-m2@4a8 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_mpu_m2_ck";
		clocks = <&dpll_mpu_ck>;
		ti,max-div = <31>;
		reg = <0x04a8>;
		ti,index-starts-at-one;
	};

	dpll_ddr_ck: clock@494 {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-no-gate-clock";
		clock-output-names = "dpll_ddr_ck";
		clocks = <&sys_clkin_ck>, <&sys_clkin_ck>;
		reg = <0x0494>, <0x0434>, <0x0440>, <0x0438>, <0x043c>;
	};

	dpll_ddr_m2_ck: clock-dpll-ddr-m2@4a0 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_ddr_m2_ck";
		clocks = <&dpll_ddr_ck>;
		ti,max-div = <31>;
		reg = <0x04a0>;
		ti,index-starts-at-one;
	};

	dpll_ddr_m2_div2_ck: clock-dpll-ddr-m2-div2 {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dpll_ddr_m2_div2_ck";
		clocks = <&dpll_ddr_m2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	dpll_disp_ck: clock@498 {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-no-gate-clock";
		clock-output-names = "dpll_disp_ck";
		clocks = <&sys_clkin_ck>, <&sys_clkin_ck>;
		reg = <0x0498>, <0x0448>, <0x0454>, <0x044c>, <0x0450>;
	};

	dpll_disp_m2_ck: clock-dpll-disp-m2@4a4 {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_disp_m2_ck";
		clocks = <&dpll_disp_ck>;
		ti,max-div = <31>;
		reg = <0x04a4>;
		ti,index-starts-at-one;
		ti,set-rate-parent;
	};

	dpll_per_ck: clock@48c {
		#clock-cells = <0>;
		compatible = "ti,am3-dpll-no-gate-j-type-clock";
		clock-output-names = "dpll_per_ck";
		clocks = <&sys_clkin_ck>, <&sys_clkin_ck>;
		reg = <0x048c>, <0x0470>, <0x049c>, <0x0474>, <0x0478>;
	};

	dpll_per_m2_ck: clock-dpll-per-m2@4ac {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clock-output-names = "dpll_per_m2_ck";
		clocks = <&dpll_per_ck>;
		ti,max-div = <31>;
		reg = <0x04ac>;
		ti,index-starts-at-one;
	};

	dpll_per_m2_div4_wkupdm_ck: clock-dpll-per-m2-div4-wkupdm {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dpll_per_m2_div4_wkupdm_ck";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <4>;
	};

	dpll_per_m2_div4_ck: clock-dpll-per-m2-div4 {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dpll_per_m2_div4_ck";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <4>;
	};

	clk_24mhz: clock-clk-24mhz {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "clk_24mhz";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <8>;
	};

	clkdiv32k_ck: clock-clkdiv32k {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "clkdiv32k_ck";
		clocks = <&clk_24mhz>;
		clock-mult = <1>;
		clock-div = <732>;
	};

	l3_gclk: clock-l3-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l3_gclk";
		clocks = <&dpll_core_m4_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	pruss_ocp_gclk: clock-pruss-ocp-gclk@530 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "pruss_ocp_gclk";
		clocks = <&l3_gclk>, <&dpll_disp_m2_ck>;
		reg = <0x0530>;
	};

	mmu_fck: clock-mmu-fck-1@914 {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clock-output-names = "mmu_fck";
		clocks = <&dpll_core_m4_ck>;
		ti,bit-shift = <1>;
		reg = <0x0914>;
	};

	timer1_fck: clock-timer1-fck@528 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer1_fck";
		clocks = <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>, <&tclkin_ck>, <&clk_rc32k_ck>, <&clk_32768_ck>;
		reg = <0x0528>;
	};

	timer2_fck: clock-timer2-fck@508 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer2_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x0508>;
	};

	timer3_fck: clock-timer3-fck@50c {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer3_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x050c>;
	};

	timer4_fck: clock-timer4-fck@510 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer4_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x0510>;
	};

	timer5_fck: clock-timer5-fck@518 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer5_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x0518>;
	};

	timer6_fck: clock-timer6-fck@51c {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer6_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x051c>;
	};

	timer7_fck: clock-timer7-fck@504 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "timer7_fck";
		clocks = <&tclkin_ck>, <&sys_clkin_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x0504>;
	};

	usbotg_fck: clock-usbotg-fck-8@47c {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clock-output-names = "usbotg_fck";
		clocks = <&dpll_per_ck>;
		ti,bit-shift = <8>;
		reg = <0x047c>;
	};

	dpll_core_m4_div2_ck: clock-dpll-core-m4-div2 {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "dpll_core_m4_div2_ck";
		clocks = <&dpll_core_m4_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	ieee5000_fck: clock-ieee5000-fck-1@e4 {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clock-output-names = "ieee5000_fck";
		clocks = <&dpll_core_m4_div2_ck>;
		ti,bit-shift = <1>;
		reg = <0x00e4>;
	};

	wdt1_fck: clock-wdt1-fck@538 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "wdt1_fck";
		clocks = <&clk_rc32k_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x0538>;
	};

	l4_rtc_gclk: clock-l4-rtc-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l4_rtc_gclk";
		clocks = <&dpll_core_m4_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	l4hs_gclk: clock-l4hs-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l4hs_gclk";
		clocks = <&dpll_core_m4_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	l3s_gclk: clock-l3s-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l3s_gclk";
		clocks = <&dpll_core_m4_div2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	l4fw_gclk: clock-l4fw-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l4fw_gclk";
		clocks = <&dpll_core_m4_div2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	l4ls_gclk: clock-l4ls-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "l4ls_gclk";
		clocks = <&dpll_core_m4_div2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	sysclk_div_ck: clock-sysclk-div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "sysclk_div_ck";
		clocks = <&dpll_core_m4_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	cpsw_125mhz_gclk: clock-cpsw-125mhz-gclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "cpsw_125mhz_gclk";
		clocks = <&dpll_core_m5_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	cpsw_cpts_rft_clk: clock-cpsw-cpts-rft@520 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "cpsw_cpts_rft_clk";
		clocks = <&dpll_core_m5_ck>, <&dpll_core_m4_ck>;
		reg = <0x0520>;
	};

	gpio0_dbclk_mux_ck: clock-gpio0-dbclk-mux@53c {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "gpio0_dbclk_mux_ck";
		clocks = <&clk_rc32k_ck>, <&clk_32768_ck>, <&clk_24mhz_clkctrl AM3_CLK_24MHZ_CLKDIV32K_CLKCTRL 0>;
		reg = <0x053c>;
	};

	lcd_gclk: clock-lcd-gclk@534 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clock-output-names = "lcd_gclk";
		clocks = <&dpll_disp_m2_ck>, <&dpll_core_m5_ck>, <&dpll_per_m2_ck>;
		reg = <0x0534>;
		ti,set-rate-parent;
	};

	mmc_clk: clock-mmc {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clock-output-names = "mmc_clk";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	clock@52c {
		compatible = "ti,clksel";
		reg = <0x52c>;
		#clock-cells = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		gfx_fclk_clksel_ck: clock-gfx-fclk-clksel@1 {
			reg = <1>;
			#clock-cells = <0>;
			compatible = "ti,mux-clock";
			clock-output-names = "gfx_fclk_clksel_ck";
			clocks = <&dpll_core_m4_ck>, <&dpll_per_m2_ck>;
		};

		gfx_fck_div_ck: clock-gfx-fck-div@0 {
			reg = <0>;
			#clock-cells = <0>;
			compatible = "ti,divider-clock";
			clock-output-names = "gfx_fck_div_ck";
			clocks = <&gfx_fclk_clksel_ck>;
			ti,max-div = <2>;
		};
	};

	clock@700 {
		compatible = "ti,clksel";
		reg = <0x700>;
		#clock-cells = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		sysclkout_pre_ck: clock-sysclkout-pre@0 {
			reg = <0>;
			#clock-cells = <0>;
			compatible = "ti,mux-clock";
			clock-output-names = "sysclkout_pre_ck";
			clocks = <&clk_32768_ck>, <&l3_gclk>, <&dpll_ddr_m2_ck>, <&dpll_per_m2_ck>, <&lcd_gclk>;
		};

		clkout2_div_ck: clock-clkout2-div@3 {
			reg = <3>;
			#clock-cells = <0>;
			compatible = "ti,divider-clock";
			clock-output-names = "clkout2_div_ck";
			clocks = <&sysclkout_pre_ck>;
			ti,max-div = <8>;
		};

		clkout2_ck: clock-clkout2@7 {
			reg = <7>;
			#clock-cells = <0>;
			compatible = "ti,gate-clock";
			clock-output-names = "clkout2_ck";
			clocks = <&clkout2_div_ck>;
		};
	};
};

&prcm {
	per_cm: clock@0 {
		compatible = "ti,omap4-cm";
		clock-output-names = "per_cm";
		reg = <0x0 0x400>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x0 0x400>;

		l4ls_clkctrl: clock@38 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4ls_clkctrl";
			reg = <0x38 0x2c>, <0x6c 0x28>, <0xac 0xc>, <0xc0 0x1c>, <0xec 0xc>, <0x10c 0x8>, <0x130 0x4>;
			#clock-cells = <2>;
		};

		l3s_clkctrl: clock@1c {
			compatible = "ti,clkctrl";
			clock-output-names = "l3s_clkctrl";
			reg = <0x1c 0x4>, <0x30 0x8>, <0x68 0x4>, <0xf8 0x4>;
			#clock-cells = <2>;
		};

		l3_clkctrl: clock@24 {
			compatible = "ti,clkctrl";
			clock-output-names = "l3_clkctrl";
			reg = <0x24 0xc>, <0x94 0x10>, <0xbc 0x4>, <0xdc 0x8>, <0xfc 0x8>;
			#clock-cells = <2>;
		};

		l4hs_clkctrl: clock@120 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4hs_clkctrl";
			reg = <0x120 0x4>;
			#clock-cells = <2>;
		};

		pruss_ocp_clkctrl: clock@e8 {
			compatible = "ti,clkctrl";
			clock-output-names = "pruss_ocp_clkctrl";
			reg = <0xe8 0x4>;
			#clock-cells = <2>;
		};

		cpsw_125mhz_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "cpsw_125mhz_clkctrl";
			reg = <0x0 0x18>;
			#clock-cells = <2>;
		};

		lcdc_clkctrl: clock@18 {
			compatible = "ti,clkctrl";
			clock-output-names = "lcdc_clkctrl";
			reg = <0x18 0x4>;
			#clock-cells = <2>;
		};

		clk_24mhz_clkctrl: clock@14c {
			compatible = "ti,clkctrl";
			clock-output-names = "clk_24mhz_clkctrl";
			reg = <0x14c 0x4>;
			#clock-cells = <2>;
		};
	};

	wkup_cm: clock@400 {
		compatible = "ti,omap4-cm";
		clock-output-names = "wkup_cm";
		reg = <0x400 0x100>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x400 0x100>;

		l4_wkup_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4_wkup_clkctrl";
			reg = <0x0 0x10>, <0xb4 0x24>;
			#clock-cells = <2>;
		};

		l3_aon_clkctrl: clock@14 {
			compatible = "ti,clkctrl";
			clock-output-names = "l3_aon_clkctrl";
			reg = <0x14 0x4>;
			#clock-cells = <2>;
		};

		l4_wkup_aon_clkctrl: clock@b0 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4_wkup_aon_clkctrl";
			reg = <0xb0 0x4>;
			#clock-cells = <2>;
		};
	};

	mpu_cm: clock@600 {
		compatible = "ti,omap4-cm";
		clock-output-names = "mpu_cm";
		reg = <0x600 0x100>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x600 0x100>;

		mpu_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "mpu_clkctrl";
			reg = <0x0 0x8>;
			#clock-cells = <2>;
		};
	};

	l4_rtc_cm: clock@800 {
		compatible = "ti,omap4-cm";
		clock-output-names = "l4_rtc_cm";
		reg = <0x800 0x100>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x800 0x100>;

		l4_rtc_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4_rtc_clkctrl";
			reg = <0x0 0x4>;
			#clock-cells = <2>;
		};
	};

	gfx_l3_cm: clock@900 {
		compatible = "ti,omap4-cm";
		clock-output-names = "gfx_l3_cm";
		reg = <0x900 0x100>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x900 0x100>;

		gfx_l3_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "gfx_l3_clkctrl";
			reg = <0x0 0x8>;
			#clock-cells = <2>;
		};
	};

	l4_cefuse_cm: clock@a00 {
		compatible = "ti,omap4-cm";
		clock-output-names = "l4_cefuse_cm";
		reg = <0xa00 0x100>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0xa00 0x100>;

		l4_cefuse_clkctrl: clock@0 {
			compatible = "ti,clkctrl";
			clock-output-names = "l4_cefuse_clkctrl";
			reg = <0x0 0x24>;
			#clock-cells = <2>;
		};
	};
};
