// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include "tegra124-nyan.dtsi"

#include "tegra124-nyan-big-emc.dtsi"

/ {
	model = "Acer Chromebook 13 CB5-311";
	compatible = "google,nyan-big-rev7", "google,nyan-big-rev6",
		     "google,nyan-big-rev5", "google,nyan-big-rev4",
		     "google,nyan-big-rev3", "google,nyan-big-rev2",
		     "google,nyan-big-rev1", "google,nyan-big-rev0",
		     "google,nyan-big", "google,nyan", "nvidia,tegra124";

	host1x@50000000 {
		dpaux@545c0000 {
			aux-bus {
				panel: panel {
					compatible = "auo,b133xtn01";
					power-supply = <&vdd_3v3_panel>;
					backlight = <&backlight>;
				};
			};
		};
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_default>;

		pinmux_default: pinmux {
			clk_32k_out_pa0 {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart3_cts_n_pa1 {
				nvidia,pins = "uart3_cts_n_pa1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap2_fs_pa2 {
				nvidia,pins = "dap2_fs_pa2";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap2_sclk_pa3 {
				nvidia,pins = "dap2_sclk_pa3";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap2_din_pa4 {
				nvidia,pins = "dap2_din_pa4";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap2_dout_pa5 {
				nvidia,pins = "dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_clk_pa6 {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_cmd_pa7 {
				nvidia,pins = "sdmmc3_cmd_pa7";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pb0 {
				nvidia,pins = "pb0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pb1 {
				nvidia,pins = "pb1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_dat3_pb4 {
				nvidia,pins = "sdmmc3_dat3_pb4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat2_pb5 {
				nvidia,pins = "sdmmc3_dat2_pb5";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat1_pb6 {
				nvidia,pins = "sdmmc3_dat1_pb6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat0_pb7 {
				nvidia,pins = "sdmmc3_dat0_pb7";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart3_rts_n_pc0 {
				nvidia,pins = "uart3_rts_n_pc0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_txd_pc2 {
				nvidia,pins = "uart2_txd_pc2";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_rxd_pc3 {
				nvidia,pins = "uart2_rxd_pc3";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gen1_i2c_scl_pc4 {
				nvidia,pins = "gen1_i2c_scl_pc4";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			gen1_i2c_sda_pc5 {
				nvidia,pins = "gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pc7 {
				nvidia,pins = "pc7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg0 {
				nvidia,pins = "pg0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg1 {
				nvidia,pins = "pg1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg2 {
				nvidia,pins = "pg2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg3 {
				nvidia,pins = "pg3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg4 {
				nvidia,pins = "pg4";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg5 {
				nvidia,pins = "pg5";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg6 {
				nvidia,pins = "pg6";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg7 {
				nvidia,pins = "pg7";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph0 {
				nvidia,pins = "ph0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph1 {
				nvidia,pins = "ph1";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph2 {
				nvidia,pins = "ph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph3 {
				nvidia,pins = "ph3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph4 {
				nvidia,pins = "ph4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph5 {
				nvidia,pins = "ph5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph6 {
				nvidia,pins = "ph6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph7 {
				nvidia,pins = "ph7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi0 {
				nvidia,pins = "pi0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi1 {
				nvidia,pins = "pi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi2 {
				nvidia,pins = "pi2";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi3 {
				nvidia,pins = "pi3";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi4 {
				nvidia,pins = "pi4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi5 {
				nvidia,pins = "pi5";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi6 {
				nvidia,pins = "pi6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi7 {
				nvidia,pins = "pi7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pj0 {
				nvidia,pins = "pj0";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pj2 {
				nvidia,pins = "pj2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_cts_n_pj5 {
				nvidia,pins = "uart2_cts_n_pj5";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_rts_n_pj6 {
				nvidia,pins = "uart2_rts_n_pj6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pj7 {
				nvidia,pins = "pj7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pk0 {
				nvidia,pins = "pk0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk1 {
				nvidia,pins = "pk1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk2 {
				nvidia,pins = "pk2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pk3 {
				nvidia,pins = "pk3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk4 {
				nvidia,pins = "pk4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_out_pk5 {
				nvidia,pins = "spdif_out_pk5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_in_pk6 {
				nvidia,pins = "spdif_in_pk6";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk7 {
				nvidia,pins = "pk7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap1_fs_pn0 {
				nvidia,pins = "dap1_fs_pn0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_din_pn1 {
				nvidia,pins = "dap1_din_pn1";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_dout_pn2 {
				nvidia,pins = "dap1_dout_pn2";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_sclk_pn3 {
				nvidia,pins = "dap1_sclk_pn3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			usb_vbus_en0_pn4 {
				nvidia,pins = "usb_vbus_en0_pn4";
				nvidia,function = "usb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			usb_vbus_en1_pn5 {
				nvidia,pins = "usb_vbus_en1_pn5";
				nvidia,function = "usb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			hdmi_int_pn7 {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data7_po0 {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data0_po1 {
				nvidia,pins = "ulpi_data0_po1";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data1_po2 {
				nvidia,pins = "ulpi_data1_po2";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data2_po3 {
				nvidia,pins = "ulpi_data2_po3";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data3_po4 {
				nvidia,pins = "ulpi_data3_po4";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data4_po5 {
				nvidia,pins = "ulpi_data4_po5";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data5_po6 {
				nvidia,pins = "ulpi_data5_po6";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data6_po7 {
				nvidia,pins = "ulpi_data6_po7";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_fs_pp0 {
				nvidia,pins = "dap3_fs_pp0";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_din_pp1 {
				nvidia,pins = "dap3_din_pp1";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_dout_pp2 {
				nvidia,pins = "dap3_dout_pp2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_sclk_pp3 {
				nvidia,pins = "dap3_sclk_pp3";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_fs_pp4 {
				nvidia,pins = "dap4_fs_pp4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_din_pp5 {
				nvidia,pins = "dap4_din_pp5";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_dout_pp6 {
				nvidia,pins = "dap4_dout_pp6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_sclk_pp7 {
				nvidia,pins = "dap4_sclk_pp7";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col0_pq0 {
				nvidia,pins = "kb_col0_pq0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col1_pq1 {
				nvidia,pins = "kb_col1_pq1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col2_pq2 {
				nvidia,pins = "kb_col2_pq2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col3_pq3 {
				nvidia,pins = "kb_col3_pq3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col4_pq4 {
				nvidia,pins = "kb_col4_pq4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col5_pq5 {
				nvidia,pins = "kb_col5_pq5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col6_pq6 {
				nvidia,pins = "kb_col6_pq6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col7_pq7 {
				nvidia,pins = "kb_col7_pq7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row0_pr0 {
				nvidia,pins = "kb_row0_pr0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row1_pr1 {
				nvidia,pins = "kb_row1_pr1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row2_pr2 {
				nvidia,pins = "kb_row2_pr2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row3_pr3 {
				nvidia,pins = "kb_row3_pr3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row4_pr4 {
				nvidia,pins = "kb_row4_pr4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row5_pr5 {
				nvidia,pins = "kb_row5_pr5";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row6_pr6 {
				nvidia,pins = "kb_row6_pr6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row7_pr7 {
				nvidia,pins = "kb_row7_pr7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row8_ps0 {
				nvidia,pins = "kb_row8_ps0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row9_ps1 {
				nvidia,pins = "kb_row9_ps1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row10_ps2 {
				nvidia,pins = "kb_row10_ps2";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row11_ps3 {
				nvidia,pins = "kb_row11_ps3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row12_ps4 {
				nvidia,pins = "kb_row12_ps4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row13_ps5 {
				nvidia,pins = "kb_row13_ps5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row14_ps6 {
				nvidia,pins = "kb_row14_ps6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row15_ps7 {
				nvidia,pins = "kb_row15_ps7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row16_pt0 {
				nvidia,pins = "kb_row16_pt0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row17_pt1 {
				nvidia,pins = "kb_row17_pt1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gen2_i2c_scl_pt5 {
				nvidia,pins = "gen2_i2c_scl_pt5";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			gen2_i2c_sda_pt6 {
				nvidia,pins = "gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_cmd_pt7 {
				nvidia,pins = "sdmmc4_cmd_pt7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu0 {
				nvidia,pins = "pu0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pu1 {
				nvidia,pins = "pu1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pu2 {
				nvidia,pins = "pu2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pu3 {
				nvidia,pins = "pu3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pu4 {
				nvidia,pins = "pu4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu5 {
				nvidia,pins = "pu5";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu6 {
				nvidia,pins = "pu6";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pv0 {
				nvidia,pins = "pv0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pv1 {
				nvidia,pins = "pv1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_cd_n_pv2 {
				nvidia,pins = "sdmmc3_cd_n_pv2";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_wp_n_pv3 {
				nvidia,pins = "sdmmc1_wp_n_pv3";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ddc_scl_pv4 {
				nvidia,pins = "ddc_scl_pv4";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			ddc_sda_pv5 {
				nvidia,pins = "ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			gpio_w2_aud_pw2 {
				nvidia,pins = "gpio_w2_aud_pw2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_w3_aud_pw3 {
				nvidia,pins = "gpio_w3_aud_pw3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap_mclk1_pw4 {
				nvidia,pins = "dap_mclk1_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk2_out_pw5 {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart3_txd_pw6 {
				nvidia,pins = "uart3_txd_pw6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart3_rxd_pw7 {
				nvidia,pins = "uart3_rxd_pw7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dvfs_pwm_px0 {
				nvidia,pins = "dvfs_pwm_px0";
				nvidia,function = "cldvfs";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x1_aud_px1 {
				nvidia,pins = "gpio_x1_aud_px1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dvfs_clk_px2 {
				nvidia,pins = "dvfs_clk_px2";
				nvidia,function = "cldvfs";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x3_aud_px3 {
				nvidia,pins = "gpio_x3_aud_px3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x4_aud_px4 {
				nvidia,pins = "gpio_x4_aud_px4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gpio_x5_aud_px5 {
				nvidia,pins = "gpio_x5_aud_px5";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x6_aud_px6 {
				nvidia,pins = "gpio_x6_aud_px6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x7_aud_px7 {
				nvidia,pins = "gpio_x7_aud_px7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_clk_py0 {
				nvidia,pins = "ulpi_clk_py0";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_dir_py1 {
				nvidia,pins = "ulpi_dir_py1";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_nxt_py2 {
				nvidia,pins = "ulpi_nxt_py2";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_stp_py3 {
				nvidia,pins = "ulpi_stp_py3";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat3_py4 {
				nvidia,pins = "sdmmc1_dat3_py4";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_dat2_py5 {
				nvidia,pins = "sdmmc1_dat2_py5";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_dat1_py6 {
				nvidia,pins = "sdmmc1_dat1_py6";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_dat0_py7 {
				nvidia,pins = "sdmmc1_dat0_py7";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_clk_pz0 {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_cmd_pz1 {
				nvidia,pins = "sdmmc1_cmd_pz1";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pwr_i2c_scl_pz6 {
				nvidia,pins = "pwr_i2c_scl_pz6";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pwr_i2c_sda_pz7 {
				nvidia,pins = "pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat0_paa0 {
				nvidia,pins = "sdmmc4_dat0_paa0";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat1_paa1 {
				nvidia,pins = "sdmmc4_dat1_paa1";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat2_paa2 {
				nvidia,pins = "sdmmc4_dat2_paa2";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat3_paa3 {
				nvidia,pins = "sdmmc4_dat3_paa3";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat4_paa4 {
				nvidia,pins = "sdmmc4_dat4_paa4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat5_paa5 {
				nvidia,pins = "sdmmc4_dat5_paa5";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat6_paa6 {
				nvidia,pins = "sdmmc4_dat6_paa6";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat7_paa7 {
				nvidia,pins = "sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb0 {
				nvidia,pins = "pbb0";
				nvidia,function = "vgp6";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cam_i2c_scl_pbb1 {
				nvidia,pins = "cam_i2c_scl_pbb1";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			cam_i2c_sda_pbb2 {
				nvidia,pins = "cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pbb3 {
				nvidia,pins = "pbb3";
				nvidia,function = "vgp3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb4 {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb5 {
				nvidia,pins = "pbb5";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb6 {
				nvidia,pins = "pbb6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb7 {
				nvidia,pins = "pbb7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cam_mclk_pcc0 {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pcc1 {
				nvidia,pins = "pcc1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pcc2 {
				nvidia,pins = "pcc2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc4_clk_pcc4 {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2_req_pcc5 {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l0_rst_n_pdd1 {
				nvidia,pins = "pex_l0_rst_n_pdd1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l0_clkreq_n_pdd2 {
				nvidia,pins = "pex_l0_clkreq_n_pdd2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_wake_n_pdd3 {
				nvidia,pins = "pex_wake_n_pdd3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l1_rst_n_pdd5 {
				nvidia,pins = "pex_l1_rst_n_pdd5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l1_clkreq_n_pdd6 {
				nvidia,pins = "pex_l1_clkreq_n_pdd6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk3_out_pee0 {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk3_req_pee1 {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap_mclk1_req_pee2 {
				nvidia,pins = "dap_mclk1_req_pee2";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			hdmi_cec_pee3 {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_clk_lb_out_pee4 {
				nvidia,pins = "sdmmc3_clk_lb_out_pee4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_clk_lb_in_pee5 {
				nvidia,pins = "sdmmc3_clk_lb_in_pee5";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dp_hpd_pff0 {
				nvidia,pins = "dp_hpd_pff0";
				nvidia,function = "dp";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			usb_vbus_en2_pff1 {
				nvidia,pins = "usb_vbus_en2_pff1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			pff2 {
				nvidia,pins = "pff2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			core_pwr_req {
				nvidia,pins = "core_pwr_req";
				nvidia,function = "pwron";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cpu_pwr_req {
				nvidia,pins = "cpu_pwr_req";
				nvidia,function = "cpu";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pwr_int_n {
				nvidia,pins = "pwr_int_n";
				nvidia,function = "pmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			reset_out_n {
				nvidia,pins = "reset_out_n";
				nvidia,function = "reset_out_n";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			owr {
				nvidia,pins = "owr";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			clk_32k_in {
				nvidia,pins = "clk_32k_in";
				nvidia,function = "clk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			jtag_rtck {
				nvidia,pins = "jtag_rtck";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
		};
	};

	mmc@700b0400 { /* SD Card on this bus */
		wp-gpios = <&gpio TEGRA_GPIO(Q, 4) GPIO_ACTIVE_LOW>;
	};

	sound {
		compatible = "nvidia,tegra-audio-max98090-nyan-big",
			     "nvidia,tegra-audio-max98090-nyan",
			     "nvidia,tegra-audio-max98090";
		nvidia,model = "GoogleNyanBig";
	};
};
