-- 3GPP TS 36.413 V15.5.0 (2019-03)
-- 9.3.6	Constant Definitions
-- **************************************************************
--
-- Constant definitions
--
-- **************************************************************

S1AP-Constants { 
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
eps-Access (21) modules (3) s1ap (1) version1 (1) s1ap-Constants (4) } 

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS
	ProcedureCode,
	ProtocolIE-ID

FROM S1AP-CommonDataTypes;


-- **************************************************************
--
-- Elementary Procedures
--
-- **************************************************************

id-HandoverPreparation						ProcedureCode ::= 0
id-HandoverResourceAllocation				ProcedureCode ::= 1
id-HandoverNotification						ProcedureCode ::= 2
id-PathSwitchRequest						ProcedureCode ::= 3
id-HandoverCancel							ProcedureCode ::= 4
id-E-RABSetup								ProcedureCode ::= 5
id-E-RABModify								ProcedureCode ::= 6
id-E-RABRelease								ProcedureCode ::= 7
id-E-RABReleaseIndication					ProcedureCode ::= 8
id-InitialContextSetup						ProcedureCode ::= 9
id-Paging									ProcedureCode ::= 10
id-downlinkNASTransport						ProcedureCode ::= 11
id-initialUEMessage							ProcedureCode ::= 12
id-uplinkNASTransport						ProcedureCode ::= 13
id-Reset									ProcedureCode ::= 14
id-ErrorIndication							ProcedureCode ::= 15
id-NASNonDeliveryIndication					ProcedureCode ::= 16
id-S1Setup									ProcedureCode ::= 17
id-UEContextReleaseRequest					ProcedureCode ::= 18
id-DownlinkS1cdma2000tunnelling				ProcedureCode ::= 19
id-UplinkS1cdma2000tunnelling				ProcedureCode ::= 20
id-UEContextModification					ProcedureCode ::= 21
id-UECapabilityInfoIndication				ProcedureCode ::= 22
id-UEContextRelease							ProcedureCode ::= 23
id-eNBStatusTransfer						ProcedureCode ::= 24
id-MMEStatusTransfer						ProcedureCode ::= 25
id-DeactivateTrace							ProcedureCode ::= 26
id-TraceStart								ProcedureCode ::= 27
id-TraceFailureIndication					ProcedureCode ::= 28
id-ENBConfigurationUpdate					ProcedureCode ::= 29
id-MMEConfigurationUpdate					ProcedureCode ::= 30
id-LocationReportingControl					ProcedureCode ::= 31
id-LocationReportingFailureIndication		ProcedureCode ::= 32
id-LocationReport							ProcedureCode ::= 33
id-OverloadStart							ProcedureCode ::= 34
id-OverloadStop								ProcedureCode ::= 35
id-WriteReplaceWarning						ProcedureCode ::= 36
id-eNBDirectInformationTransfer				ProcedureCode ::= 37
id-MMEDirectInformationTransfer				ProcedureCode ::= 38
id-PrivateMessage							ProcedureCode ::= 39
id-eNBConfigurationTransfer					ProcedureCode ::= 40
id-MMEConfigurationTransfer					ProcedureCode ::= 41
id-CellTrafficTrace							ProcedureCode ::= 42
id-Kill										ProcedureCode ::= 43
id-downlinkUEAssociatedLPPaTransport		ProcedureCode ::= 44
id-uplinkUEAssociatedLPPaTransport			ProcedureCode ::= 45
id-downlinkNonUEAssociatedLPPaTransport		ProcedureCode ::= 46
id-uplinkNonUEAssociatedLPPaTransport		ProcedureCode ::= 47
id-UERadioCapabilityMatch					ProcedureCode ::= 48
id-PWSRestartIndication						ProcedureCode ::= 49
id-E-RABModificationIndication				ProcedureCode ::= 50
id-PWSFailureIndication						ProcedureCode ::= 51
id-RerouteNASRequest						ProcedureCode ::= 52
id-UEContextModificationIndication			ProcedureCode ::= 53
id-ConnectionEstablishmentIndication		ProcedureCode ::= 54
id-UEContextSuspend							ProcedureCode ::= 55
id-UEContextResume							ProcedureCode ::= 56
id-NASDeliveryIndication					ProcedureCode ::= 57
id-RetrieveUEInformation					ProcedureCode ::= 58
id-UEInformationTransfer					ProcedureCode ::= 59
id-eNBCPRelocationIndication				ProcedureCode ::= 60
id-MMECPRelocationIndication				ProcedureCode ::= 61
id-SecondaryRATDataUsageReport				ProcedureCode ::= 62

-- **************************************************************
--
-- Extension constants
--
-- **************************************************************

maxPrivateIEs							INTEGER ::= 65535
maxProtocolExtensions					INTEGER ::= 65535
maxProtocolIEs							INTEGER ::= 65535
-- **************************************************************
--
-- Lists
--
-- **************************************************************

maxnoofCSGs								INTEGER ::= 256
maxnoofE-RABs							INTEGER ::= 256
maxnoofTAIs								INTEGER ::= 256
maxnoofTACs								INTEGER ::= 256
maxnoofErrors							INTEGER ::= 256
maxnoofBPLMNs							INTEGER ::= 6
maxnoofPLMNsPerMME						INTEGER ::= 32
maxnoofEPLMNs							INTEGER ::= 15
maxnoofEPLMNsPlusOne					INTEGER ::= 16
maxnoofForbLACs							INTEGER ::= 4096
maxnoofForbTACs							INTEGER ::= 4096
maxnoofIndividualS1ConnectionsToReset	INTEGER ::= 256
maxnoofCellsinUEHistoryInfo				INTEGER ::= 16
maxnoofCellsineNB						INTEGER ::= 256
maxnoofTAIforWarning					INTEGER ::= 65535 
maxnoofCellID							INTEGER ::= 65535 
maxnoofDCNs								INTEGER ::= 32 
maxnoofEmergencyAreaID					INTEGER ::= 65535 
maxnoofCellinTAI						INTEGER ::= 65535 
maxnoofCellinEAI						INTEGER ::= 65535 
maxnoofeNBX2TLAs						INTEGER ::= 2
maxnoofeNBX2ExtTLAs						INTEGER ::= 16
maxnoofeNBX2GTPTLAs						INTEGER ::= 16
maxnoofRATs								INTEGER ::= 8
maxnoofGroupIDs							INTEGER ::= 65535
maxnoofMMECs							INTEGER ::= 256
maxnoofCellIDforMDT						INTEGER ::= 32
maxnoofTAforMDT							INTEGER ::= 8
maxnoofMDTPLMNs							INTEGER ::= 16
maxnoofCellsforRestart					INTEGER ::= 256
maxnoofRestartTAIs						INTEGER ::= 2048
maxnoofRestartEmergencyAreaIDs			INTEGER ::= 256
maxEARFCN								INTEGER ::= 262143
maxnoofMBSFNAreaMDT						INTEGER ::= 8
maxnoofRecommendedCells					INTEGER ::= 16
maxnoofRecommendedENBs					INTEGER ::= 16
maxnooftimeperiods						INTEGER ::= 2 
maxnoofCellIDforQMC						INTEGER ::= 32
maxnoofTAforQMC							INTEGER ::= 8
maxnoofPLMNforQMC						INTEGER ::= 16
maxnoofBluetoothName					INTEGER ::= 4
maxnoofWLANName							INTEGER ::= 4
maxnoofConnectedengNBs					INTEGER ::= 256



-- **************************************************************
--
-- IEs
--
-- **************************************************************

id-MME-UE-S1AP-ID									ProtocolIE-ID ::= 0
id-HandoverType										ProtocolIE-ID ::= 1
id-Cause											ProtocolIE-ID ::= 2
id-SourceID											ProtocolIE-ID ::= 3
id-TargetID											ProtocolIE-ID ::= 4
--WS extension
id-Unknown-5										ProtocolIE-ID ::= 5
id-Unknown-6										ProtocolIE-ID ::= 6
id-Unknown-7										ProtocolIE-ID ::= 7
id-eNB-UE-S1AP-ID									ProtocolIE-ID ::= 8
--WS extension
id-Unknown-9										ProtocolIE-ID ::= 9
id-Unknown-10										ProtocolIE-ID ::= 10
id-Unknown-11										ProtocolIE-ID ::= 11
id-E-RABSubjecttoDataForwardingList					ProtocolIE-ID ::= 12
id-E-RABtoReleaseListHOCmd							ProtocolIE-ID ::= 13
id-E-RABDataForwardingItem							ProtocolIE-ID ::= 14
id-E-RABReleaseItemBearerRelComp					ProtocolIE-ID ::= 15
id-E-RABToBeSetupListBearerSUReq					ProtocolIE-ID ::= 16
id-E-RABToBeSetupItemBearerSUReq					ProtocolIE-ID ::= 17
id-E-RABAdmittedList								ProtocolIE-ID ::= 18
id-E-RABFailedToSetupListHOReqAck					ProtocolIE-ID ::= 19
id-E-RABAdmittedItem								ProtocolIE-ID ::= 20
id-E-RABFailedtoSetupItemHOReqAck					ProtocolIE-ID ::= 21
id-E-RABToBeSwitchedDLList							ProtocolIE-ID ::= 22
id-E-RABToBeSwitchedDLItem							ProtocolIE-ID ::= 23
id-E-RABToBeSetupListCtxtSUReq						ProtocolIE-ID ::= 24
id-TraceActivation									ProtocolIE-ID ::= 25
id-NAS-PDU											ProtocolIE-ID ::= 26
id-E-RABToBeSetupItemHOReq							ProtocolIE-ID ::= 27
id-E-RABSetupListBearerSURes						ProtocolIE-ID ::= 28
id-E-RABFailedToSetupListBearerSURes				ProtocolIE-ID ::= 29
id-E-RABToBeModifiedListBearerModReq				ProtocolIE-ID ::= 30
id-E-RABModifyListBearerModRes						ProtocolIE-ID ::= 31
id-E-RABFailedToModifyList							ProtocolIE-ID ::= 32
id-E-RABToBeReleasedList							ProtocolIE-ID ::= 33
id-E-RABFailedToReleaseList							ProtocolIE-ID ::= 34
id-E-RABItem										ProtocolIE-ID ::= 35
id-E-RABToBeModifiedItemBearerModReq				ProtocolIE-ID ::= 36
id-E-RABModifyItemBearerModRes						ProtocolIE-ID ::= 37
id-E-RABReleaseItem									ProtocolIE-ID ::= 38
id-E-RABSetupItemBearerSURes						ProtocolIE-ID ::= 39
id-SecurityContext									ProtocolIE-ID ::= 40
id-HandoverRestrictionList							ProtocolIE-ID ::= 41
--WS extension
id-Unknown-42										ProtocolIE-ID ::= 42
id-UEPagingID										ProtocolIE-ID ::= 43
id-pagingDRX										ProtocolIE-ID ::= 44
--WS extension
id-Unknown-45										ProtocolIE-ID ::= 45
id-TAIList											ProtocolIE-ID ::= 46
id-TAIItem											ProtocolIE-ID ::= 47
id-E-RABFailedToSetupListCtxtSURes					ProtocolIE-ID ::= 48
id-E-RABReleaseItemHOCmd							ProtocolIE-ID ::= 49
id-E-RABSetupItemCtxtSURes							ProtocolIE-ID ::= 50
id-E-RABSetupListCtxtSURes							ProtocolIE-ID ::= 51
id-E-RABToBeSetupItemCtxtSUReq						ProtocolIE-ID ::= 52
id-E-RABToBeSetupListHOReq							ProtocolIE-ID ::= 53
--WS extension
id-Unknown-54										ProtocolIE-ID ::= 54
id-GERANtoLTEHOInformationRes						ProtocolIE-ID ::= 55
--WS extension
id-Unknown-56										ProtocolIE-ID ::= 56
id-UTRANtoLTEHOInformationRes						ProtocolIE-ID ::= 57
id-CriticalityDiagnostics 							ProtocolIE-ID ::= 58
id-Global-ENB-ID									ProtocolIE-ID ::= 59
id-eNBname											ProtocolIE-ID ::= 60
id-MMEname											ProtocolIE-ID ::= 61
--WS extension
id-Unknown-62										ProtocolIE-ID ::= 62
id-ServedPLMNs										ProtocolIE-ID ::= 63
id-SupportedTAs										ProtocolIE-ID ::= 64
id-TimeToWait										ProtocolIE-ID ::= 65
id-uEaggregateMaximumBitrate						ProtocolIE-ID ::= 66
id-TAI												ProtocolIE-ID ::= 67
--WS extension
id-Unknown-68										ProtocolIE-ID ::= 68
id-E-RABReleaseListBearerRelComp					ProtocolIE-ID ::= 69
id-cdma2000PDU										ProtocolIE-ID ::= 70
id-cdma2000RATType									ProtocolIE-ID ::= 71
id-cdma2000SectorID									ProtocolIE-ID ::= 72
id-SecurityKey										ProtocolIE-ID ::= 73
id-UERadioCapability								ProtocolIE-ID ::= 74
id-GUMMEI-ID										ProtocolIE-ID ::= 75
--WS extension
id-Unknown-76										ProtocolIE-ID ::= 76
id-Unknown-77										ProtocolIE-ID ::= 77
id-E-RABInformationListItem							ProtocolIE-ID ::= 78
id-Direct-Forwarding-Path-Availability				ProtocolIE-ID ::= 79
id-UEIdentityIndexValue								ProtocolIE-ID ::= 80
--WS extension
id-Unknown-81										ProtocolIE-ID ::= 81
id-Unknown-82										ProtocolIE-ID ::= 82
id-cdma2000HOStatus									ProtocolIE-ID ::= 83
id-cdma2000HORequiredIndication						ProtocolIE-ID ::= 84
--WS extension
id-Unknown-85										ProtocolIE-ID ::= 85
id-E-UTRAN-Trace-ID									ProtocolIE-ID ::= 86
id-RelativeMMECapacity								ProtocolIE-ID ::= 87
id-SourceMME-UE-S1AP-ID								ProtocolIE-ID ::= 88
id-Bearers-SubjectToStatusTransfer-Item				ProtocolIE-ID ::= 89
id-eNB-StatusTransfer-TransparentContainer			ProtocolIE-ID ::= 90
id-UE-associatedLogicalS1-ConnectionItem			ProtocolIE-ID ::= 91
id-ResetType										ProtocolIE-ID ::= 92
id-UE-associatedLogicalS1-ConnectionListResAck		ProtocolIE-ID ::= 93
id-E-RABToBeSwitchedULItem							ProtocolIE-ID ::= 94
id-E-RABToBeSwitchedULList							ProtocolIE-ID ::= 95
id-S-TMSI											ProtocolIE-ID ::= 96
id-cdma2000OneXRAND									ProtocolIE-ID ::= 97
id-RequestType										ProtocolIE-ID ::= 98
id-UE-S1AP-IDs										ProtocolIE-ID ::= 99
id-EUTRAN-CGI										ProtocolIE-ID ::= 100
id-OverloadResponse									ProtocolIE-ID ::= 101
id-cdma2000OneXSRVCCInfo							ProtocolIE-ID ::= 102
id-E-RABFailedToBeReleasedList						ProtocolIE-ID ::= 103
id-Source-ToTarget-TransparentContainer				ProtocolIE-ID ::= 104
id-ServedGUMMEIs									ProtocolIE-ID ::= 105
id-SubscriberProfileIDforRFP						ProtocolIE-ID ::= 106
id-UESecurityCapabilities							ProtocolIE-ID ::= 107
id-CSFallbackIndicator								ProtocolIE-ID ::= 108
id-CNDomain											ProtocolIE-ID ::= 109
id-E-RABReleasedList								ProtocolIE-ID ::= 110
id-MessageIdentifier								ProtocolIE-ID ::= 111
id-SerialNumber										ProtocolIE-ID ::= 112
id-WarningAreaList									ProtocolIE-ID ::= 113
id-RepetitionPeriod									ProtocolIE-ID ::= 114
id-NumberofBroadcastRequest							ProtocolIE-ID ::= 115
id-WarningType										ProtocolIE-ID ::= 116
id-WarningSecurityInfo								ProtocolIE-ID ::= 117
id-DataCodingScheme									ProtocolIE-ID ::= 118
id-WarningMessageContents							ProtocolIE-ID ::= 119
id-BroadcastCompletedAreaList						ProtocolIE-ID ::= 120
id-Inter-SystemInformationTransferTypeEDT			ProtocolIE-ID ::= 121
id-Inter-SystemInformationTransferTypeMDT			ProtocolIE-ID ::= 122
id-Target-ToSource-TransparentContainer				ProtocolIE-ID ::= 123
id-SRVCCOperationPossible							ProtocolIE-ID ::= 124
id-SRVCCHOIndication								ProtocolIE-ID ::= 125
id-NAS-DownlinkCount								ProtocolIE-ID ::= 126
id-CSG-Id											ProtocolIE-ID ::= 127
id-CSG-IdList										ProtocolIE-ID ::= 128
id-SONConfigurationTransferECT						ProtocolIE-ID ::= 129
id-SONConfigurationTransferMCT						ProtocolIE-ID ::= 130
id-TraceCollectionEntityIPAddress					ProtocolIE-ID ::= 131
id-MSClassmark2										ProtocolIE-ID ::= 132
id-MSClassmark3										ProtocolIE-ID ::= 133
id-RRC-Establishment-Cause							ProtocolIE-ID ::= 134
id-NASSecurityParametersfromE-UTRAN					ProtocolIE-ID ::= 135
id-NASSecurityParameterstoE-UTRAN					ProtocolIE-ID ::= 136
id-DefaultPagingDRX									ProtocolIE-ID ::= 137
id-Source-ToTarget-TransparentContainer-Secondary	ProtocolIE-ID ::= 138
id-Target-ToSource-TransparentContainer-Secondary	ProtocolIE-ID ::= 139
id-EUTRANRoundTripDelayEstimationInfo				ProtocolIE-ID ::= 140
id-BroadcastCancelledAreaList						ProtocolIE-ID ::= 141
id-ConcurrentWarningMessageIndicator				ProtocolIE-ID ::= 142
id-Data-Forwarding-Not-Possible						ProtocolIE-ID ::= 143
id-ExtendedRepetitionPeriod							ProtocolIE-ID ::= 144
id-CellAccessMode									ProtocolIE-ID ::= 145
id-CSGMembershipStatus 								ProtocolIE-ID ::= 146
id-LPPa-PDU											ProtocolIE-ID ::= 147
id-Routing-ID										ProtocolIE-ID ::= 148
id-Time-Synchronisation-Info							ProtocolIE-ID ::= 149
id-PS-ServiceNotAvailable							ProtocolIE-ID ::= 150
id-PagingPriority									ProtocolIE-ID ::= 151
id-x2TNLConfigurationInfo							ProtocolIE-ID ::= 152
id-eNBX2ExtendedTransportLayerAddresses				ProtocolIE-ID ::= 153
id-GUMMEIList										ProtocolIE-ID ::= 154
id-GW-TransportLayerAddress							ProtocolIE-ID ::= 155
id-Correlation-ID									ProtocolIE-ID ::= 156
id-SourceMME-GUMMEI									ProtocolIE-ID ::= 157
id-MME-UE-S1AP-ID-2									ProtocolIE-ID ::= 158
id-RegisteredLAI									ProtocolIE-ID ::= 159
id-RelayNode-Indicator								ProtocolIE-ID ::= 160
id-TrafficLoadReductionIndication					ProtocolIE-ID ::= 161
id-MDTConfiguration									ProtocolIE-ID ::= 162
id-MMERelaySupportIndicator							ProtocolIE-ID ::= 163
id-GWContextReleaseIndication						ProtocolIE-ID ::= 164
id-ManagementBasedMDTAllowed						ProtocolIE-ID ::= 165
id-PrivacyIndicator									ProtocolIE-ID ::= 166
id-Time-UE-StayedInCell-EnhancedGranularity			ProtocolIE-ID ::= 167
id-HO-Cause											ProtocolIE-ID ::= 168
id-VoiceSupportMatchIndicator						ProtocolIE-ID ::= 169
id-GUMMEIType										ProtocolIE-ID ::= 170
id-M3Configuration									ProtocolIE-ID ::= 171
id-M4Configuration									ProtocolIE-ID ::= 172
id-M5Configuration									ProtocolIE-ID ::= 173
id-MDT-Location-Info								ProtocolIE-ID ::= 174
id-MobilityInformation								ProtocolIE-ID ::= 175
id-Tunnel-Information-for-BBF						ProtocolIE-ID ::= 176
id-ManagementBasedMDTPLMNList						ProtocolIE-ID ::= 177
id-SignallingBasedMDTPLMNList						ProtocolIE-ID ::= 178
id-ULCOUNTValueExtended								ProtocolIE-ID ::= 179
id-DLCOUNTValueExtended								ProtocolIE-ID ::= 180
id-ReceiveStatusOfULPDCPSDUsExtended				ProtocolIE-ID ::= 181
id-ECGIListForRestart								ProtocolIE-ID ::= 182
id-SIPTO-Correlation-ID								ProtocolIE-ID ::= 183
id-SIPTO-L-GW-TransportLayerAddress					ProtocolIE-ID ::= 184
id-TransportInformation								ProtocolIE-ID ::= 185
id-LHN-ID											ProtocolIE-ID ::= 186
id-AdditionalCSFallbackIndicator					ProtocolIE-ID ::= 187
id-TAIListForRestart								ProtocolIE-ID ::= 188
id-UserLocationInformation							ProtocolIE-ID ::= 189
id-EmergencyAreaIDListForRestart					ProtocolIE-ID ::= 190
id-KillAllWarningMessages							ProtocolIE-ID ::= 191
id-Masked-IMEISV									ProtocolIE-ID ::= 192
id-eNBIndirectX2TransportLayerAddresses				ProtocolIE-ID ::= 193
id-uE-HistoryInformationFromTheUE					ProtocolIE-ID ::= 194
id-ProSeAuthorized									ProtocolIE-ID ::= 195
id-ExpectedUEBehaviour								ProtocolIE-ID ::= 196
id-LoggedMBSFNMDT									ProtocolIE-ID ::= 197
id-UERadioCapabilityForPaging						ProtocolIE-ID ::= 198
id-E-RABToBeModifiedListBearerModInd				ProtocolIE-ID ::= 199
id-E-RABToBeModifiedItemBearerModInd				ProtocolIE-ID ::= 200
id-E-RABNotToBeModifiedListBearerModInd				ProtocolIE-ID ::= 201
id-E-RABNotToBeModifiedItemBearerModInd				ProtocolIE-ID ::= 202
id-E-RABModifyListBearerModConf						ProtocolIE-ID ::= 203
id-E-RABModifyItemBearerModConf						ProtocolIE-ID ::= 204
id-E-RABFailedToModifyListBearerModConf				ProtocolIE-ID ::= 205
id-SON-Information-Report							ProtocolIE-ID ::= 206
id-Muting-Availability-Indication					ProtocolIE-ID ::= 207
id-Muting-Pattern-Information						ProtocolIE-ID ::= 208
id-Synchronisation-Information						ProtocolIE-ID ::= 209
id-E-RABToBeReleasedListBearerModConf				ProtocolIE-ID ::= 210
id-AssistanceDataForPaging							ProtocolIE-ID ::= 211
id-CellIdentifierAndCELevelForCECapableUEs			ProtocolIE-ID ::= 212
id-InformationOnRecommendedCellsAndENBsForPaging	ProtocolIE-ID ::= 213
id-RecommendedCellItem								ProtocolIE-ID ::= 214
id-RecommendedENBItem								ProtocolIE-ID ::= 215
id-ProSeUEtoNetworkRelaying							ProtocolIE-ID ::= 216
id-ULCOUNTValuePDCP-SNlength18						ProtocolIE-ID ::= 217
id-DLCOUNTValuePDCP-SNlength18						ProtocolIE-ID ::= 218
id-ReceiveStatusOfULPDCPSDUsPDCP-SNlength18			ProtocolIE-ID ::= 219
id-M6Configuration									ProtocolIE-ID ::= 220
id-M7Configuration									ProtocolIE-ID ::= 221
id-PWSfailedECGIList								ProtocolIE-ID ::= 222
id-MME-Group-ID										ProtocolIE-ID ::= 223
id-Additional-GUTI									ProtocolIE-ID ::= 224
id-S1-Message										ProtocolIE-ID ::= 225
id-CSGMembershipInfo								ProtocolIE-ID ::= 226
id-Paging-eDRXInformation							ProtocolIE-ID ::= 227
id-UE-RetentionInformation							ProtocolIE-ID ::= 228
--WS extension
id-Unknown-229										ProtocolIE-ID ::= 229
id-UE-Usage-Type									ProtocolIE-ID ::= 230
id-extended-UEIdentityIndexValue					ProtocolIE-ID ::= 231
id-RAT-Type											ProtocolIE-ID ::= 232
id-BearerType										ProtocolIE-ID ::= 233
id-NB-IoT-DefaultPagingDRX							ProtocolIE-ID ::= 234
id-E-RABFailedToResumeListResumeReq					ProtocolIE-ID ::= 235
id-E-RABFailedToResumeItemResumeReq					ProtocolIE-ID ::= 236
id-E-RABFailedToResumeListResumeRes					ProtocolIE-ID ::= 237
id-E-RABFailedToResumeItemResumeRes					ProtocolIE-ID ::= 238
id-NB-IoT-Paging-eDRXInformation					ProtocolIE-ID ::= 239
id-V2XServicesAuthorized							ProtocolIE-ID ::= 240
id-UEUserPlaneCIoTSupportIndicator 					ProtocolIE-ID ::= 241
id-CE-mode-B-SupportIndicator 						ProtocolIE-ID ::= 242
id-SRVCCOperationNotPossible						ProtocolIE-ID ::= 243
id-NB-IoT-UEIdentityIndexValue 						ProtocolIE-ID ::= 244
id-RRC-Resume-Cause									ProtocolIE-ID ::= 245
id-DCN-ID											ProtocolIE-ID ::= 246
id-ServedDCNs					 					ProtocolIE-ID ::= 247
id-UESidelinkAggregateMaximumBitrate 				ProtocolIE-ID ::= 248
id-DLNASPDUDeliveryAckRequest						ProtocolIE-ID ::= 249
id-Coverage-Level 									ProtocolIE-ID ::= 250
id-EnhancedCoverageRestricted						ProtocolIE-ID ::= 251
id-UE-Level-QoS-Parameters							ProtocolIE-ID ::= 252
id-DL-CP-SecurityInformation						ProtocolIE-ID ::= 253
id-UL-CP-SecurityInformation						ProtocolIE-ID ::= 254
id-extended-e-RAB-MaximumBitrateDL					ProtocolIE-ID ::= 255
id-extended-e-RAB-MaximumBitrateUL					ProtocolIE-ID ::= 256
id-extended-e-RAB-GuaranteedBitrateDL				ProtocolIE-ID ::= 257
id-extended-e-RAB-GuaranteedBitrateUL				ProtocolIE-ID ::= 258
id-extended-uEaggregateMaximumBitRateDL				ProtocolIE-ID ::= 259
id-extended-uEaggregateMaximumBitRateUL				ProtocolIE-ID ::= 260
id-NRrestrictioninEPSasSecondaryRAT					ProtocolIE-ID ::= 261
id-UEAppLayerMeasConfig								ProtocolIE-ID ::= 262
id-UE-Application-Layer-Measurement-Capability		ProtocolIE-ID ::= 263
id-SecondaryRATDataUsageReportList					ProtocolIE-ID ::= 264
id-SecondaryRATDataUsageReportItem					ProtocolIE-ID ::= 265
id-HandoverFlag										ProtocolIE-ID ::= 266
id-E-RABUsageReportItem								ProtocolIE-ID ::= 267
id-SecondaryRATDataUsageRequest						ProtocolIE-ID ::= 268
id-NRUESecurityCapabilities							ProtocolIE-ID ::= 269
id-UnlicensedSpectrumRestriction					ProtocolIE-ID ::= 270
id-CE-ModeBRestricted								ProtocolIE-ID ::= 271
id-LTE-M-Indication									ProtocolIE-ID ::= 272
id-DownlinkPacketLossRate							ProtocolIE-ID ::= 273
id-UplinkPacketLossRate								ProtocolIE-ID ::= 274
id-UECapabilityInfoRequest							ProtocolIE-ID ::= 275
id-serviceType										ProtocolIE-ID ::= 276
id-AerialUEsubscriptionInformation					ProtocolIE-ID ::= 277
id-Subscription-Based-UE-DifferentiationInfo		ProtocolIE-ID ::= 278
--WS extension
id-Unknown-279										ProtocolIE-ID ::= 279
id-EndIndication									ProtocolIE-ID ::= 280
id-EDT-Session										ProtocolIE-ID ::= 281
id-CNTypeRestrictions								ProtocolIE-ID ::= 282
id-PendingDataIndication							ProtocolIE-ID ::= 283
id-BluetoothMeasurementConfiguration				ProtocolIE-ID ::= 284
id-WLANMeasurementConfiguration						ProtocolIE-ID ::= 285
id-WarningAreaCoordinates							ProtocolIE-ID ::= 286
id-NRrestrictionin5GS								ProtocolIE-ID ::= 287
id-PSCellInformation								ProtocolIE-ID ::= 288
--WS extension
id-Unknown-289									ProtocolIE-ID ::= 289
id-LastNG-RANPLMNIdentity							ProtocolIE-ID ::= 290
id-ConnectedengNBList								ProtocolIE-ID ::= 291
id-ConnectedengNBToAddList							ProtocolIE-ID ::= 292
id-ConnectedengNBToRemoveList						ProtocolIE-ID ::= 293
id-EN-DCSONConfigurationTransfer-ECT				ProtocolIE-ID ::= 294
id-EN-DCSONConfigurationTransfer-MCT				ProtocolIE-ID ::= 295

END
