<?xml version="1.0" encoding="UTF-8"?>
<section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>Common Commands</title>
  <para>These commands are available on all VTY nodes. They are listed here only once, to unclutter the VTY reference.</para>
  <section>
    <title>end</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>end</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>end</para>
          <para>End current mode and change to enable mode.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>exit</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>exit</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>exit</para>
          <para>Exit current mode and down to previous mode</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>help</para>
          <para>Description of the interactive help system</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>list [with-flags]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>list [with-flags]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>list</para>
          <para>Print command list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[with-flags]</para>
          <para>Also print the VTY attribute flags</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show running-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show running-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>running-config</para>
          <para>running configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show vty-attributes</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show vty-attributes</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty-attributes</para>
          <para>List of VTY attributes</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show vty-attributes (application|library|global)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show vty-attributes (application|library|global)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty-attributes</para>
          <para>List of VTY attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application specific attributes only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>library</para>
          <para>Library specific attributes only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global attributes only</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write file [PATH]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write file [PATH]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Write to configuration file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[PATH]</para>
          <para>Set file path to store the config, or replace if already exists</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write memory</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write memory</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>memory</para>
          <para>Write configuration to the file (same as write file)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write terminal</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write terminal</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Write to terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>view</title>
  <para>The view node is the default node when connecting to the
    VTY interface. This node does not require any additional
    permission and allows to introspect the application.</para>
  <section>
    <title>enable [expert-mode]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable [expert-mode]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Turn on privileged mode command</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[expert-mode]</para>
          <para>Enable the expert mode (show hidden commands)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging enable</title>
    <para>This command is required to make logging commands available
      on the telnet VTY.</para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loa...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging set-log-mask MASK</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging set-log-mask MASK</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-log-mask</para>
          <para>Set the logmask of this logging target</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|ls...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal) .LOGMESSAGE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logp</para>
          <para>Print a message on all log outputs; useful for placing markers in test logs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.LOGMESSAGE</para>
          <para>Arbitrary message to log on given category and log level</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show asciidoc counters</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show asciidoc counters</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asciidoc</para>
          <para>Asciidoc generation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>counters</para>
          <para>Generate table of all registered counters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cpu-sched threads</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cpu-sched threads</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Show Sched section information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>threads</para>
          <para>Show information about running threads)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>config</para>
          <para>Currently running cs7 configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Display all active ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display all ASs (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>Display all m3ua ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>Display all SUA ASs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association status</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[all-matches]</para>
          <para>Display all matching Combination Links</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [lis...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route-lookup</para>
          <para>Look up route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>from</para>
          <para>From</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Origin PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls</para>
          <para>SLS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SLS value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[list-asps]</para>
          <para>List ASPs of the AS if route points to an AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp addressbook</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp addressbook</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>addressbook</para>
          <para>List all SCCP addressbook entries</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp connections</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp connections</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>connections</para>
          <para>Show List of active SCCP connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Find an SCCP User registered for the given SSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Subsystem Number (SSN)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp timers</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp timers</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signaling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timers</para>
          <para>Show List of SCCP timers</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>Show List of SCCP Users registered</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>User Table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm</para>
          <para>Show information about finite state machines</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Display information about a single named finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm</para>
          <para>Show information about finite state machines</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display a list of all registered finite state machines</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-instances NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-instances NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-instances</para>
          <para>Show information about finite state machine instances</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Display a list of all FSM instances of the named finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-instances all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-instances all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-instances</para>
          <para>Show information about finite state machine instances</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display a list of all FSM instances of all finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-state-graph NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-state-graph NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-state-graph</para>
          <para>Generate a state transition graph (using DOT language)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>FSM name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show logging vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show logging vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Show current logging configuration for this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show online-help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show online-help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>online-help</para>
          <para>Online help</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show pid</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show pid</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pid</para>
          <para>Displays the process ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show rate-counters [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show rate-counters [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rate-counters</para>
          <para>Show all rate counters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show runtime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show runtime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>runtime</para>
          <para>Display runtime information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats level (global|peer|subscriber) [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats level (global|peer|subscriber) [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Show global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Show global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter chunks using regular expression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>REGEXP</para>
          <para>Regular expression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tree</para>
          <para>Display only a specific memory chunk</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDRESS</para>
          <para>Chunk address (e.g. 0xdeadbeef)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show uptime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show uptime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>uptime</para>
          <para>Displays how long the program has been running</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show version</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show version</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>version</para>
          <para>Displays program version</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines on screen (0 for no pausing)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no length</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no length</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>who</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>who</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>who</para>
          <para>Display who is on vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>enable</title>
  <para>The enable node is a privileged node, allowing to make changes
    to the configuration and to access further commands like 'configure'.
    All commands seen on the view node are also available here.</para>
  <section>
    <title>configure [terminal]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>configure [terminal]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>configure</para>
          <para>Configuration from vty interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[terminal]</para>
          <para>Configuration terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>copy running-config startup-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>copy running-config startup-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>copy</para>
          <para>Copy configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>running-config</para>
          <para>Copy running config to... </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>startup-config</para>
          <para>Copy running config to startup config (same as write file)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt; asp NAME audit point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt; asp NAME audit point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Instance related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SS7 Instance Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>audit</para>
          <para>Audit destination Point Code (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Destination Point Code to audit</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination Point Code value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt; asp NAME disconnect</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt; asp NAME disconnect</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Instance related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SS7 Instance Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disconnect</para>
          <para>Disconnect the ASP (client will reconnect)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Turn off privileged mode command</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging enable</title>
    <para>This command is required to make logging commands available
      on the telnet VTY.</para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loa...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging set-log-mask MASK</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging set-log-mask MASK</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-log-mask</para>
          <para>Set the logmask of this logging target</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|ls...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal) .LOGMESSAGE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logp</para>
          <para>Print a message on all log outputs; useful for placing markers in test logs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.LOGMESSAGE</para>
          <para>Arbitrary message to log on given category and log level</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show asciidoc counters</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show asciidoc counters</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asciidoc</para>
          <para>Asciidoc generation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>counters</para>
          <para>Generate table of all registered counters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cpu-sched threads</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cpu-sched threads</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Show Sched section information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>threads</para>
          <para>Show information about running threads)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>config</para>
          <para>Currently running cs7 configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Display all active ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display all ASs (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>Display all m3ua ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>Display all SUA ASs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association status</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[all-matches]</para>
          <para>Display all matching Combination Links</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [lis...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route-lookup</para>
          <para>Look up route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>from</para>
          <para>From</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Origin PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls</para>
          <para>SLS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SLS value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[list-asps]</para>
          <para>List ASPs of the AS if route points to an AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp addressbook</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp addressbook</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>addressbook</para>
          <para>List all SCCP addressbook entries</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp connections</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp connections</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>connections</para>
          <para>Show List of active SCCP connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Find an SCCP User registered for the given SSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Subsystem Number (SSN)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp timers</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp timers</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signaling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timers</para>
          <para>Show List of SCCP timers</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>Show List of SCCP Users registered</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>User Table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm</para>
          <para>Show information about finite state machines</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Display information about a single named finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm</para>
          <para>Show information about finite state machines</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display a list of all registered finite state machines</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-instances NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-instances NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-instances</para>
          <para>Show information about finite state machine instances</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Display a list of all FSM instances of the named finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-instances all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-instances all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-instances</para>
          <para>Show information about finite state machine instances</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display a list of all FSM instances of all finite state machine</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show fsm-state-graph NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show fsm-state-graph NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fsm-state-graph</para>
          <para>Generate a state transition graph (using DOT language)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>FSM name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show logging vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show logging vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Show current logging configuration for this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show online-help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show online-help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>online-help</para>
          <para>Online help</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show rate-counters [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show rate-counters [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rate-counters</para>
          <para>Show all rate counters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show runtime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show runtime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>runtime</para>
          <para>Display runtime information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show startup-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show startup-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>startup-config</para>
          <para>Contentes of startup configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats level (global|peer|subscriber) [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats level (global|peer|subscriber) [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Show global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Show global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter chunks using regular expression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>REGEXP</para>
          <para>Regular expression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tree</para>
          <para>Display only a specific memory chunk</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDRESS</para>
          <para>Chunk address (e.g. 0xdeadbeef)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show version</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show version</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>version</para>
          <para>Displays program version</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Request a shutdown of the program</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats report</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats report</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Stats related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>report</para>
          <para>Manurally trigger reporting of stats</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Stats related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Reset all rate counter stats</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines on screen (0 for no pausing)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal monitor</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal monitor</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>monitor</para>
          <para>Copy debug output to the current terminal line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no length</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no length</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no monitor</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no monitor</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>monitor</para>
          <para>Copy debug output to the current terminal line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>who</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>who</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>who</para>
          <para>Display who is on vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config</title>
  <para>The config node is the root for all configuration commands,
    which are identical to the config file format. Changes made on the telnet
    VTY can be made persistent with the 'write file' command.</para>
  <section>
    <title>banner motd default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>banner motd default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner string</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Strings for motd</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Default string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>banner motd file [FILE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>banner motd file [FILE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Banner for motd</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Banner from a file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[FILE]</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cpu-sched</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cpu-sched</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Configure CPU Scheduler related settings</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Configure a SS7 Instance</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable password (8|) WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable password (8|) WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>8</para>
          <para>Specifies a HIDDEN password will follow</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para/>
          <para>dummy string </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>The HIDDEN 'enable' password string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable password LINE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable password LINE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>LINE</para>
          <para>The UNENCRYPTED (cleartext) 'enable' password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>hostname WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>hostname WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>hostname</para>
          <para>Set system's network name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>This system's network name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>line vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>line vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>line</para>
          <para>Configure a terminal line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Virtual terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log alarms &lt;2-32700&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log alarms &lt;2-32700&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Logging alarms to osmo_strrb</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;2-32700&gt;</para>
          <para>Maximum number of messages to log</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log file FILENAME [blocking-io]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log file FILENAME [blocking-io]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Logging to text file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>FILENAME</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[blocking-io]</para>
          <para>Use blocking, synchronous I/O</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log gsmtap [HOSTNAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log gsmtap [HOSTNAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsmtap</para>
          <para>Logging via GSMTAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name to send the GSMTAP logging to (UDP port 4729)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log stderr [blocking-io]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log stderr [blocking-io]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stderr</para>
          <para>Logging via STDERR of the process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[blocking-io]</para>
          <para>Use blocking, synchronous I/O</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>authpriv</para>
          <para>Security/authorization messages facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cron</para>
          <para>Clock daemon (cron/at) facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daemon</para>
          <para>General system daemon facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ftp</para>
          <para>Ftp daemon facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpr</para>
          <para>Line printer facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mail</para>
          <para>Mail facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>news</para>
          <para>News facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user</para>
          <para>Generic facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>uucp</para>
          <para>UUCP facility</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log syslog local &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log syslog local &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local</para>
          <para>Syslog LOCAL facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>Local facility number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log systemd-journal [raw]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log systemd-journal [raw]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>systemd-journal</para>
          <para>Logging to systemd-journal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[raw]</para>
          <para>Offload rendering of the meta information (location, category) to systemd</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no banner motd</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no banner motd</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner string</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Strings for motd</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no enable password</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no enable password</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no hostname [HOSTNAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no hostname [HOSTNAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>hostname</para>
          <para>Reset system's network name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name of this router</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Logging alarms to osmo_strrb</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log file FILENAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log file FILENAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Logging to text file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>FILENAME</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log gsmtap [HOSTNAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log gsmtap [HOSTNAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsmtap</para>
          <para>Logging via GSMTAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name to send the GSMTAP logging to (UDP port 4729)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log stderr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log stderr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stderr</para>
          <para>Logging via STDERR of the process</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log syslog</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log syslog</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log systemd-journal</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log systemd-journal</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>systemd-journal</para>
          <para>Logging to systemd-journal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no service advanced-vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no service advanced-vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>advanced-vty</para>
          <para>Enable advanced mode vty interface</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no service terminal-length [&lt;0-512&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no service terminal-length [&lt;0-512&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal-length</para>
          <para>System wide terminal length configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-512&gt;]</para>
          <para>Number of lines of VTY (0 means no line control)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no stats reporter log [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no stats reporter log [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Report to the logger</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no stats reporter statsd [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no stats reporter statsd [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>statsd</para>
          <para>Report to a STATSD server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>password (8|) WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>password (8|) WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the terminal connection password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>8</para>
          <para>Specifies a HIDDEN password will follow</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para/>
          <para>dummy string </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>The HIDDEN line password string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>password LINE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>password LINE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the terminal connection password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>LINE</para>
          <para>The UNENCRYPTED (cleartext) line password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>service advanced-vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>service advanced-vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>advanced-vty</para>
          <para>Enable advanced mode vty interface</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>service terminal-length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>service terminal-length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal-length</para>
          <para>System wide terminal length configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines of VTY (0 means no line control)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats interval &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats interval &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>interval</para>
          <para>Set the reporting interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Interval in seconds (0 disables the reporting interval)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reporter log [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reporter log [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Report to the logger</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reporter statsd [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reporter statsd [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>statsd</para>
          <para>Report to a STATSD server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats-tcp batch-size &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats-tcp batch-size &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats-tcp</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>batch-size</para>
          <para>Set the number of tcp sockets that are processed per stats polling interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Number of sockets per interval</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats-tcp interval &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats-tcp interval &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats-tcp</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>interval</para>
          <para>Set the tcp socket stats polling interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Interval in seconds (0 disables the polling interval)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-log</title>
  <para>The log node is commonly available in all Osmocom programs and
    allows configuring logging to stderr and/or log files, including logging
    category and level filtering as well as output formatting options.
    Note that the 'logging enable' command is required to make logging commands
    available on the telnet VTY.</para>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loa...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-stats</title>
  <para/>
  <section>
    <title>disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disable the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enable the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>flush-period &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>flush-period &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>flush-period</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Send all stats even if they have not changed (i.e. force the flush)every N-th reporting interval. Set to 0 to disable regular flush (default).</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>level (global|peer|subscriber)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>level (global|peer|subscriber)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Report global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Report global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Report global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip ADDR</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip ADDR</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Set the IP address to which we bind locally</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDR</para>
          <para>IP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>mtu &lt;100-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>mtu &lt;100-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mtu</para>
          <para>Set the maximum packet size</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;100-65535&gt;</para>
          <para>Size in byte</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Set the IP address to which we bind locally</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no mtu</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no mtu</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mtu</para>
          <para>Set the maximum packet size</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no prefix</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no prefix</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>prefix</para>
          <para>Set the item name prefix</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>prefix PREFIX</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>prefix PREFIX</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>prefix</para>
          <para>Set the item name prefix</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PREFIX</para>
          <para>The prefix string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-ip ADDR</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-ip ADDR</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Set the remote IP address to which we connect</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDR</para>
          <para>IP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-port &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-port &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-port</para>
          <para>Set the remote port to which we connect</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-line</title>
  <para/>
  <section>
    <title>bind A.B.C.D [&lt;0-65535&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bind A.B.C.D [&lt;0-65535&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>Accept VTY telnet connections on local interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local interface IP address (default: 127.0.0.1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65535&gt;]</para>
          <para>Local TCP port number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>login</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>login</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>login</para>
          <para>Enable password checking</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no login</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no login</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>login</para>
          <para>Enable password checking</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7</title>
  <para/>
  <section>
    <title>as NAME (sua|m3ua|ipa)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>as NAME (sua|m3ua|ipa)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Configure an Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Configure Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Local port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa) (sctp|tcp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa) (sctp|tcp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Configure Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Local port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Configure/Enable xUA Listener</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65534&gt;</para>
          <para>Port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sctp]</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[tcp]</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>network-indicator (international | national | reserved | spare)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>network-indicator (international | national | reserved | spare)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>network-indicator</para>
          <para>Configure the Network Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>international</para>
          <para>International Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>national</para>
          <para>National Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reserved</para>
          <para>Reserved Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>spare</para>
          <para>Spare Network</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no as NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no as NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Disable Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Disable Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Disable xUA Listener on given port</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65534&gt;</para>
          <para>Port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sctp]</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[tcp]</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sccp-address NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sccp-address NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-address</para>
          <para>Delete an SCCP addressbook entry</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the SCCP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Configure the local Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code delimiter (default|dash)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code delimiter (default|dash)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>delimiter</para>
          <para>Configure Point Code Delimiter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Use dot as delimiter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dash</para>
          <para>User dash as delimiter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>format</para>
          <para>Configure Point Code Format</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-24&gt;</para>
          <para>Length of first PC component</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;1-23&gt;]</para>
          <para>Length of second PC component</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;1-22&gt;]</para>
          <para>Length of third PC component</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code format default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code format default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>format</para>
          <para>Configure Point Code Format</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Default Point Code Format (3.8.3)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>route-table system</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>route-table system</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route-table</para>
          <para>Specify the name of the route table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>system</para>
          <para>Name of the route table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp max-optional-data (&lt;0-999999&gt;|standard)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp max-optional-data (&lt;0-999999&gt;|standard)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Configure SCCP behavior</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-optional-data</para>
          <para>Adjust the upper bound for the optional data length (the payload) for CR, CC, CREF and RLSD messages. For any Optional Data part larger than this value in octets, send CR, CC, CREF and RLSD messages without any payload, and send the data payload in a separate Data Form 1 message. ITU-T Q.713 sections 4.2 thru 4.5 define a limit of 128 bytes for the 'Data' parameter. This limit can be adjusted here. May be useful for interop with nonstandard SCCP peers.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999999&gt;</para>
          <para>Set a non-standard maximum allowed number of bytes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>standard</para>
          <para>Use the ITU-T Q.713 4.2 to 4.5 standard value of 128</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp-address NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp-address NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-address</para>
          <para>Create/Modify an SCCP addressbook entry</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the SCCP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-99999...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-timer</para>
          <para>Configure SCCP timer values, see ITU-T Q.714</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>conn_est</para>
          <para>Waiting for connection confirm message, 1 to 2 minutes (default: 60)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ias</para>
          <para>Send keep-alive: on an idle connection, delay before sending an Idle Timer message, 5 to 10 minutes (default: 420)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>iar</para>
          <para>Receive keep-alive: on an idle connection, delay until considering a connection as stale, 11 to 21 minutes (default: 900)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rel</para>
          <para>Waiting for release complete message, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>repeat_rel</para>
          <para>Waiting for release complete message; or to repeat sending released message after the initial expiry, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>int</para>
          <para>Waiting for release complete message; or to release connection resources, freeze the LRN and alert a maintenance function after the initial expiry, extending to 1 minute (default: 60)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>guard</para>
          <para>Waiting to resume normal procedure for temporary connection sections during the restart procedure, 23 to 25 minutes (default: 1380)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Waiting to release temporary connection section or alert maintenance function after reset request message is sent, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reassembly</para>
          <para>Waiting to receive all the segments of the remaining segments, single segmented message after receiving the first segment, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>secondary-pc POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>secondary-pc POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>secondary-pc</para>
          <para>Configure the local Secondary Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-opc-dpc [opc-shift] [&lt;0-8&gt;] [dpc-shift] [&lt;0-8&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-opc-dpc [opc-shift] [&lt;0-8&gt;] [dpc-shift] [&lt;0-8&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-opc-dpc</para>
          <para>Shift OPC and DPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-shift]</para>
          <para>Shift OPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-8&gt;]</para>
          <para>How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[dpc-shift]</para>
          <para>Shift DPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-8&gt;]</para>
          <para>How many bits from ITU DPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-shift &lt;0-6&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-shift &lt;0-6&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-shift</para>
          <para>Shift SLS bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-6&gt;</para>
          <para>How many bits from derivated 7-bit extended-SLS (OPC, DPC, SLS) field (starting from least-significant-bit) to skip</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>xua rkm routing-key-allocation (static-only|dynamic-permitted)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>xua rkm routing-key-allocation (static-only|dynamic-permitted)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xua</para>
          <para>SIGTRAN xxxUA related</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rkm</para>
          <para>Routing Key Management</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key-allocation</para>
          <para>Routing Key Management Allocation Policy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>static-only</para>
          <para>Only static (pre-configured) Routing Keys permitted</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dynamic-permitted</para>
          <para>Dynamically allocate Routing Keys for what ASPs request</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-as</title>
  <para/>
  <section>
    <title>asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Specify that a given ASP is part of this AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP to be added to AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>binding-table reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>binding-table reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>AS Loadshare binding table operations</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Reset loadshare binding table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Specify ASP to be removed from this AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP to be removed</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no point-code override (opc|dpc)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no point-code override (opc|dpc)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code of messages received at the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>opc</para>
          <para>Override Source Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dpc</para>
          <para>Override Destination Point Code of received messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no traffic-mode</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no traffic-mode</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Remove explicit traffic mode of operation of this AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code override (opc|dpc) PC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code override (opc|dpc) PC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code of messages received at the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>opc</para>
          <para>Override Source Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dpc</para>
          <para>Override Destination Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PC</para>
          <para>New Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code override patch-sccp (disabled|both)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code override patch-sccp (disabled|both)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code to hard-coded value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>patch-sccp</para>
          <para>Patch point code values into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disabled</para>
          <para>Don't patch any point codes into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>both</para>
          <para>Patch both origin and destination point codes into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>qos-class &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>qos-class &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>qos-class</para>
          <para>Specity QoS Class of AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>QoS Class</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>recovery-timeout &lt;1-2000&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>recovery-timeout &lt;1-2000&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>recovery-timeout</para>
          <para>Specifies RFC4666 recovery timer T(r) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-2000&gt;</para>
          <para>Recovery Timeout in Milliseconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>si</para>
          <para>Match on Service Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>aal2</para>
          <para>ATM Adaption Layer 2</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bicc</para>
          <para>Bearer Independent Call Control</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>b-isup</para>
          <para>Broadband ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>h248</para>
          <para>H.248</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>isup</para>
          <para>ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sat-isup</para>
          <para>Sattelite ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tup</para>
          <para>Telephony User Part</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn S...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn SSN</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>si</para>
          <para>Match on Service Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>aal2</para>
          <para>ATM Adaption Layer 2</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bicc</para>
          <para>Bearer Independent Call Control</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>b-isup</para>
          <para>Broadband ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>h248</para>
          <para>H.248</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>isup</para>
          <para>ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sat-isup</para>
          <para>Sattelite ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tup</para>
          <para>Telephony User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Match on Sub-System Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>SSN</para>
          <para>Sub-System Number to match on</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC ssn SSN</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC ssn SSN</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Match on Sub-System Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>SSN</para>
          <para>Sub-System Number to match on</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-shift &lt;0-3&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-shift &lt;0-3&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-shift</para>
          <para>Shift SLS bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-3&gt;</para>
          <para>How many bits from SLS field (starting from least-significant-bit) to skip</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>traffic-mode (broadcast | roundrobin | override)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>traffic-mode (broadcast | roundrobin | override)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Specifies traffic mode of operation of the ASP within the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>broadcast</para>
          <para>Broadcast to all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>roundrobin</para>
          <para>Round-Robin between all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>traffic-mode (loadshare|loadshare-tcap) [bindings] [sls] [opc-sls] [opc-shift] [...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>traffic-mode (loadshare|loadshare-tcap) [bindings] [sls] [opc-sls] [opc-shift] [&lt;0-2&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Specifies traffic mode of operation of the ASP within the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loadshare</para>
          <para>Share Load among all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loadshare-tcap</para>
          <para>Share Load among all ASP within AS (TCAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[bindings]</para>
          <para>Configure Loadshare parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sls]</para>
          <para>Configure Loadshare SLS generation parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-sls]</para>
          <para>Generate extended SLS with OPC information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-shift]</para>
          <para>Shift OPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2&gt;]</para>
          <para>How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-asp</title>
  <para/>
  <section>
    <title>block</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>block</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>block</para>
          <para>Allows a SCTP Association with ASP, but doesn't let it become active</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>destination-audit asp-active</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>destination-audit asp-active</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>destination-audit</para>
          <para>Configure ASP Auditing (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-active</para>
          <para>Transmit DAUD after ASP successful activate (for remote PCs in sccp address-book)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip (A.B.C.D|X:X::X:X) [primary]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip (A.B.C.D|X:X::X:X) [primary]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Specify Local IP Address from which to contact ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IPv4 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Local IPv6 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[primary]</para>
          <para>Signal the SCTP peer to use this address as Primary Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no destination-audit asp-active</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no destination-audit asp-active</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>destination-audit</para>
          <para>Configure ASP Auditing (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-active</para>
          <para>Transmit xUA DAUD after ASP successful activate (for remote PCs in sccp address-book)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Specify Local IP Address from which to contact ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IPv4 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Local IPv6 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no quirk (no_notify|daud_in_asp|snm_inactive)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no quirk (no_notify|daud_in_asp|snm_inactive)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>quirk</para>
          <para>Disable quirk to work around interop issues</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no_notify</para>
          <para>Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daud_in_asp</para>
          <para>Allow Rx of DAUD in ASP role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>snm_inactive</para>
          <para>Allow Rx of [S]SNM in AS-INACTIVE state</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no remote-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no remote-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Specify Remote IP Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sctp-param init (num-ostreams|max-instreams|max-attempts|timeout)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sctp-param init (num-ostreams|max-instreams|max-attempts|timeout)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-attempts</para>
          <para>Configure INIT Maximum Attempts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timeout</para>
          <para>Configure INIT Timeout (milliseconds)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Terminates SCTP association; New associations will be rejected</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param keepalive</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param keepalive</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param keepalive (time|intvl|probes)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param keepalive (time|intvl|probes)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>time</para>
          <para>Configure number of seconds a connection needs to be idle before beggining to send probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>intvl</para>
          <para>Configure number of seconds between probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>probes</para>
          <para>Configure max number of probes to send before giving up if no response is obtained</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param user-timeout</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param user-timeout</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user-timeout</para>
          <para>Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>qos-class &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>qos-class &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>qos-class</para>
          <para>Specify QoS Class of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>QoS Class</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>quirk (no_notify|daud_in_asp|snm_inactive)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>quirk (no_notify|daud_in_asp|snm_inactive)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>quirk</para>
          <para>Enable quirk to work around interop issues</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no_notify</para>
          <para>Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daud_in_asp</para>
          <para>Allow Rx of DAUD in ASP role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>snm_inactive</para>
          <para>Allow Rx of [S]SNM in AS-INACTIVE state</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-ip (A.B.C.D|X:X::X:X) [primary]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-ip (A.B.C.D|X:X::X:X) [primary]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Specify Remote IP Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[primary]</para>
          <para>Set remote address as SCTP Primary Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>role (sg|asp|ipsp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>role (sg|asp|ipsp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>role</para>
          <para>Specify the xUA role for this ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sg</para>
          <para>SG (Signaling Gateway)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP (Application Server Process)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipsp</para>
          <para>IPSP (IP Signalling Point)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sctp-param init (num-ostreams|max-instreams|max-attempts|timeout) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sctp-param init (num-ostreams|max-instreams|max-attempts|timeout) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-attempts</para>
          <para>Configure INIT Maximum Attempts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timeout</para>
          <para>Configure INIT Timeout (milliseconds)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Terminates SCTP association; New associations will be rejected</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param keepalive (time|intvl|probes) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param keepalive (time|intvl|probes) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>time</para>
          <para>Configure number of seconds a connection needs to be idle before beggining to send probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>intvl</para>
          <para>Configure number of seconds between probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>probes</para>
          <para>Configure max number of probes to send before giving up if no response is obtained</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param keepalive enabled</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param keepalive enabled</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enabled</para>
          <para>Enable TCP keep-alive</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param user-timeout &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param user-timeout &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user-timeout</para>
          <para>Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer lm (wait_asp_up|wait_notify|wait_notify_rkm|wait_rk_reg_resp) &lt;1-999999&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer lm (wait_asp_up|wait_notify|wait_notify_rkm|wait_rk_reg_resp) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure ASP default timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm</para>
          <para>Configure ASP default lm timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_asp_up</para>
          <para>Restart ASP after timeout waiting for ASP UP (SG role) / ASP UP ACK (ASP role) (s) (default: 20)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_notify</para>
          <para>Restart ASP after timeout waiting for NOTIFY (s) (default: 2)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_notify_rkm</para>
          <para>Restart ASP after timeout waiting for NOTIFY after RKM registration (s) (default: 20)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_rk_reg_resp</para>
          <para>Restart ASP after timeout waiting for RK_REG_RESP (s) (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer xua (ack|beat) &lt;1-999999&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer xua (ack|beat) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure ASP default timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xua</para>
          <para>Configure ASP default xua timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ack</para>
          <para>Resend ASP Up/Down/Active/Inactive after timeout waiting for ASP Up/Down/Active/Inactive ACK (ASP role)(s) (default: 2)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>beat</para>
          <para>Heartbeat Timer (0 = disabled) (s) (default: 30)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>transport-role (client|server)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>transport-role (client|server)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>transport-role</para>
          <para>Specify the transport layer role for this ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>client</para>
          <para>Operate as a client; connect to a server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>server</para>
          <para>Operate as a server; wait for client connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-listen</title>
  <para/>
  <section>
    <title>accept-asp-connections (pre-configured|dynamic-permitted)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>accept-asp-connections (pre-configured|dynamic-permitted)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-asp-connections</para>
          <para>Define what kind of ASP connections to accept</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pre-configured</para>
          <para>Accept only pre-configured ASPs (source IP/port)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dynamic-permitted</para>
          <para>Accept any connection and dynamically create an ASP definition</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Configure the Local IP Address for xUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address to use for XUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>IPv6 Address to use for XUA</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Configure the Local IP Address for xUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address to use for XUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>IPv6 Address to use for XUA</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sctp-param init (num-ostreams|max-instreams)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sctp-param init (num-ostreams|max-instreams)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sctp-param init (num-ostreams|max-instreams) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sctp-param init (num-ostreams|max-instreams) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-rt</title>
  <para/>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remove route POINT_CODE MASK</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remove route POINT_CODE MASK</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remove</para>
          <para>Remove a Route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Remove a Route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>Point Code Mask</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update route POINT_CODE MASK linkset LS_NAME [priority] [(&lt;1-9&gt;|default)] [qos-c...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update route POINT_CODE MASK linkset LS_NAME [priority] [(&lt;1-9&gt;|default)] [qos-class] [(&lt;0-7&gt;|default)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update</para>
          <para>Update the Route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Update the Route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>Point Code Mask</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linkset</para>
          <para>Specify Destination Linkset</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>LS_NAME</para>
          <para>Linkset Name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[priority]</para>
          <para>Specify Priority (lower value means higher priority)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;1-9&gt;]</para>
          <para>Priority</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[default]</para>
          <para>Default Priority (5)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[qos-class]</para>
          <para>Specify QoS Class</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-7&gt;]</para>
          <para>QoS Class</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[default]</para>
          <para>Default QoS Class (0)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-sccpaddr</title>
  <para/>
  <section>
    <title>global-title</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>global-title</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title</para>
          <para>Add/Modify Global Title</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no global-title</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no global-title</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title</para>
          <para>Remove Global Title</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no point-code</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no point-code</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Remove point-code Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no subsystem-number</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no subsystem-number</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subsystem-number</para>
          <para>Remove Subsystem Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Add point-code Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>PC</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-indicator (GT|PC|IP)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-indicator (GT|PC|IP)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-indicator</para>
          <para>Add Routing Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>GT</para>
          <para>by global-title</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PC</para>
          <para>by point-code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IP</para>
          <para>by ip-address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>subsystem-number &lt;0-4294967295&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>subsystem-number &lt;0-4294967295&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subsystem-number</para>
          <para>Add Subsystem Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4294967295&gt;</para>
          <para>SSN</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-sccpaddr-gt</title>
  <para/>
  <section>
    <title>digits DIGITS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>digits DIGITS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>digits</para>
          <para>Set Global Title Digits</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DIGITS</para>
          <para>Number digits</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>global-title-indicator &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>global-title-indicator &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title-indicator</para>
          <para>Set Global Title Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>GTI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nature-of-address-indicator &lt;0-127&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nature-of-address-indicator &lt;0-127&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nature-of-address-indicator</para>
          <para>Set Global Title Nature of Address Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-127&gt;</para>
          <para>NAI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>numbering-plan-indicator &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>numbering-plan-indicator &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>numbering-plan-indicator</para>
          <para>Set Global Title Numbering Plan Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>NPI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>translation-type &lt;0-255&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>translation-type &lt;0-255&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>translation-type</para>
          <para>Set Global Title Translation Type</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>TT</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cpu-sched</title>
  <para/>
  <section>
    <title>cpu-affinity (self|all|&lt;0-4294967295&gt;|THREADNAME) CPUHEXMASK [delay]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cpu-affinity (self|all|&lt;0-4294967295&gt;|THREADNAME) CPUHEXMASK [delay]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-affinity</para>
          <para>Set CPU affinity mask on a (group of) thread(s)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>self</para>
          <para>Set CPU affinity mask on thread running the VTY</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Set CPU affinity mask on all process' threads</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4294967295&gt;</para>
          <para>Set CPU affinity mask on a thread with specified PID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>THREADNAME</para>
          <para>Set CPU affinity mask on a thread with specified thread name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>CPUHEXMASK</para>
          <para>CPU affinity mask</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[delay]</para>
          <para>If set, delay applying the affinity mask now and let the app handle it at a later point</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>policy rr &lt;1-32&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>policy rr &lt;1-32&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>policy</para>
          <para>Set the scheduling policy to use for the process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rr</para>
          <para>Use the SCHED_RR real-time scheduling algorithm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-32&gt;</para>
          <para>Set the SCHED_RR real-time priority</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section>
