\doxysection{include/osmocom/netif/jibuf.h File Reference}
\label{jibuf_8h}\index{include/osmocom/netif/jibuf.h@{include/osmocom/netif/jibuf.h}}


Osmocom Jitter Buffer helpers.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
{\ttfamily \#include $<$stdbool.\+h$>$}\newline
{\ttfamily \#include $<$time.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/core/timer.\+h$>$}\newline
\doxysubsubsection*{Data Structures}
\begin{DoxyCompactItemize}
\item 
struct \textbf{ osmo\+\_\+jibuf}
\begin{DoxyCompactList}\small\item\em A structure representing a single instance of a jitter buffer. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsubsection*{Typedefs}
\begin{DoxyCompactItemize}
\item 
typedef void($\ast$ {\bfseries osmo\+\_\+jibuf\+\_\+dequeue\+\_\+cb}) (struct msgb $\ast$msg, void $\ast$data)
\end{DoxyCompactItemize}
\doxysubsubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
struct \textbf{ osmo\+\_\+jibuf} $\ast$ \textbf{ osmo\+\_\+jibuf\+\_\+alloc} (void $\ast$talloc\+\_\+ctx)
\begin{DoxyCompactList}\small\item\em Allocate a new jitter buffer instance. \end{DoxyCompactList}\item 
void \textbf{ osmo\+\_\+jibuf\+\_\+delete} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb)
\begin{DoxyCompactList}\small\item\em Destroy a previously allocated jitter buffer instance. \end{DoxyCompactList}\item 
int \textbf{ osmo\+\_\+jibuf\+\_\+enqueue} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb, struct msgb $\ast$msg)
\begin{DoxyCompactList}\small\item\em Try to enqueue a packet into the jitter buffer. \end{DoxyCompactList}\item 
bool \textbf{ osmo\+\_\+jibuf\+\_\+empty} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb)
\begin{DoxyCompactList}\small\item\em Check whether the jitter buffer instance has packets queued or not. \end{DoxyCompactList}\item 
void \textbf{ osmo\+\_\+jibuf\+\_\+set\+\_\+min\+\_\+delay} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb, uint32\+\_\+t min\+\_\+delay)
\begin{DoxyCompactList}\small\item\em Set minimum buffer size for the jitter buffer. \end{DoxyCompactList}\item 
void \textbf{ osmo\+\_\+jibuf\+\_\+set\+\_\+max\+\_\+delay} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb, uint32\+\_\+t max\+\_\+delay)
\begin{DoxyCompactList}\small\item\em Set maximum buffer size for the jitter buffer. \end{DoxyCompactList}\item 
void \textbf{ osmo\+\_\+jibuf\+\_\+enable\+\_\+skew\+\_\+compensation} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb, bool enable)
\begin{DoxyCompactList}\small\item\em Toggle use of skew detection and compensation mechanism. \end{DoxyCompactList}\item 
void \textbf{ osmo\+\_\+jibuf\+\_\+set\+\_\+dequeue\+\_\+cb} (struct \textbf{ osmo\+\_\+jibuf} $\ast$jb, osmo\+\_\+jibuf\+\_\+dequeue\+\_\+cb dequeue\+\_\+cb, void $\ast$cb\+\_\+data)
\begin{DoxyCompactList}\small\item\em Set dequeue callback for the jitter buffer. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Osmocom Jitter Buffer helpers. 

