libosmo-netif 1.6.0.16-c51c Osmocom network interface library

Loading...
Searching...
No Matches
Data Fields
osmux_in_handle Struct Reference
Osmocom Multiplex Protocol

one to handle all existing RTP flows More...

`#include <osmux.h>`

## Data Fields
uint8_t | osmux_seq
| Initial Osmux seqnum for each circuit, set during osmux_xfrm_input_open_circuit()
uint8_t | batch_factor
uint16_t | batch_size
struct { |
uint32_t input_rtp_msgs |
uint32_t output_osmux_msgs |
uint64_t input_rtp_bytes |
uint64_t output_osmux_bytes |
} | stats |
void(* | deliver )(struct msgb *msg, void *data)
void * | data
char * | internal_data

## Detailed Description

one to handle all existing RTP flows

The documentation for this struct was generated from the following file:

- include/osmocom/netif/osmux.h