/*###ICF### Section handled by ICF editor, don't touch! ****/
/*-Editor annotation file-*/
/* IcfEditorFile="$TOOLKIT_DIR$\config\ide\IcfEditor\a_v1_0.xml" */
/*-Specials-*/
define symbol __ICFEDIT_intvec_start__ = 0x20000000;
/*-Memory Regions-*/
define symbol __ICFEDIT_region_ROM_start__ = 0x0;
define symbol __ICFEDIT_region_ROM_end__   = 0x0;
define symbol __ICFEDIT_region_RAM_start__ = 0x20000040;
define symbol __ICFEDIT_region_RAM_end__   = 0x20007FFF;

/*-Sizes-*/
define symbol __ICFEDIT_size_cstack__   = 0x0200;
define symbol __ICFEDIT_size_heap__     = 0x000;
/**** End of ICF editor section. ###ICF###*/


define memory mem with size = 4G;
define region RAM_region   = mem:[from __ICFEDIT_region_RAM_start__   to __ICFEDIT_region_RAM_end__];

define block CSTACK    with alignment = 8, size = __ICFEDIT_size_cstack__   { };
define block HEAP      with alignment = 8, size = __ICFEDIT_size_heap__     { };

//initialize by copy { readwrite };
do not initialize  { section .noinit };

place at address mem:__ICFEDIT_intvec_start__ { section .intvec };

place at start of RAM_region { block RamTop with fixed order {readonly, section LOWEND}};
place at end of RAM_region { block RamBottom with fixed order {section HIGHSTART, readwrite, section .init,
                             block CSTACK, block HEAP}};


